EHS Adapter Compatibility with 1000i phones and DSS/LSS Consoles

* 1000i Phones
* EHSA Protocol type needs to be SIP.
* 1024idss/1048ilss and EHSA V4 can be attached at the same time.
* 1024idss/1048ilss and EHSA V2/3 cannot be attached at the same time.

Check EHS Version

